#Properties for bcc Fe

#Elastic constants (GPa)
elastic Voigt
243.30 243.30 243.30   #C11 C22 C33
145.00 145.00 145.00   #C23 C31 C12
119.00 119.00 119.00   #C44 C55 C66

#Crystallographic orientation of the block
#(this will rotate the elastic tensor accordingly)
orientation
[121]
[-101]
[1-11]
